,NominalAirFlowRate##HVAC_AIR_FLOW##LITERS_PER_SECOND,spFanSize##LENGTH##MILLIMETERS,spMaxAbsorbedCurrent##ELECTRICAL_CURRENT##AMPERES,spProjectLineURL##OTHER##,spProductCode##OTHER##,spMotorClass##OTHER##,spEasyVentProductCode##OTHER##,ExpectedServiceLife##OTHER##,NominalRotationSpeed##OTHER##,NominalStaticPressure##HVAC_PRESSURE##PASCALS,MaintenanceUnit##OTHER##,NominalTotalPressure##HVAC_PRESSURE##PASCALS,Uniclass2.0Title##OTHER##,Uniclass2.0Code##OTHER##,ProductURL##OTHER##,URL##OTHER##,UNSPSCTitle##OTHER##,UNSPSCCode##OTHER##,MaintenanceTask##OTHER##,FanMountingType##OTHER##,MotorDriveType##OTHER##,PackingCareType##OTHER##,DischargeType##OTHER##,CapacityControlType##OTHER##,MeanTimeBetweenFailure##OTHER##,RatedVoltage##ELECTRICAL_POTENTIAL##VOLTS,ContactTelephone##OTHER##,HazardousWastePerUnit##OTHER##,HazardousWaste##OTHER##,NonHazardousWastePerUnit##OTHER##,NonHazardousWaste##OTHER##,RadioactiveWastePerUnit##OTHER##,RadioactiveWaste##OTHER##,InertWastePerUnit##OTHER##,InertWaste##OTHER##,FunctionalUnitReference##OTHER##,BatchReference##OTHER##,Reference##OTHER##,OperationTemperatureRange##OTHER##,FanPowerRate##HVAC_POWER##WATTS,ShaftPowerRate##HVAC_POWER##WATTS,NominalFrequencyRange##ELECTRICAL_FREQUENCY##HERTZ,FanRotationSpeed##OTHER##,DischargePressureLoss##HVAC_PRESSURE##PASCALS,DrivePowerLoss##HVAC_POWER##WATTS,PointOfContact##OTHER##,Air Terminal Velocity Pressure##HVAC_PRESSURE##PASCALS,DischargeVelocity##HVAC_VELOCITY##METERS_PER_SECOND,MotorPosition##OTHER##,CoilPosition##OTHER##,GrossWeight##MASS##KILOGRAMS,OmniclassTitle##OTHER##,OmniclassCode##OTHER##,SerialNumber##OTHER##,NumberOfPoles##OTHER##,GlobalTradeItemNumber##OTHER##,ArticleNumber##OTHER##,MaintenanceRegulation##OTHER##,Model##OTHER##,Arrangement##OTHER##,WrappingMaterial##OTHER##,ContainerMaterial##OTHER##,spProjectName##OTHER##,spPosition##OTHER##,spElectricalPower_Solution##ELECTRICAL_POWER##WATTS,spSpecificPower_Solution##OTHER##,MasterformatTitle##OTHER##,spInletSoundPower##OTHER##,MasterformatCode##OTHER##,spOutletSoundPower##OTHER##,ModelLabel##OTHER##,spBreakOutSoundPower##OTHER##,AssemblyPlace##OTHER##,spShaftPower_Solution##ELECTRICAL_POWER##WATTS,SpecialInstructions##OTHER##,spInletSoundPressure##OTHER##,spOutletSoundPressure##OTHER##,IFCClassification##OTHER##,spBreakOutSoundPressure##OTHER##,spIdProject##OTHER##,ConductorFunction##OTHER##,spReference##OTHER##,MaintenanceFrequency##OTHER##,spRevision##OTHER##,PhotochemicalOzoneFormationPerUnit##OTHER##,PhotochemicalOzoneFormation##OTHER##,BIMElementExpiryDate##OTHER##,InstallationDate##OTHER##,WarrantyStartDate##OTHER##,WarrantyEndDate##OTHER##,AssessmentDate##OTHER##,BIMElementIssueDate##OTHER##,AcquisitionDate##OTHER##,LifeCyclePhase##OTHER##,ResourceDepletion##OTHER##,ResourceDepletionPerUnit##OTHER##,PowerFactor##ELECTRICAL_DEMAND_FACTOR##PERCENTAGE,Manufacturer##OTHER##,Exclusions##OTHER##,EutrophicationPerUnit##OTHER##,Eutrophication##OTHER##,RenewableEnergyConsumptionPerUnit##OTHER##,RenewableEnergyConsumption##OTHER##,TotalPrimaryEnergyConsumptionPerUnit##OTHER##,NonRenewableEnergyConsumptionPerUnit##OTHER##,NonRenewableEnergyConsumption##OTHER##,ContactEmail##OTHER##,FanEfficiency##OTHER##,OverallEfficiency##OTHER##,ServiceLifeDuration##OTHER##,ImpellerDiameter##LENGTH##MILLIMETERS,Throw Distance Medium Velocity##OTHER##,DirectionOfRotation##OTHER##,DischargePosition##OTHER##,StratosphericOzoneLayerDestructionPerUnit##OTHER##,StratosphericOzoneLayerDestruction##OTHER##,AssessmentDescription##OTHER##,Description##OTHER##,IP_Code##OTHER##,BarCode##OTHER##,SoundCurve##OTHER##,PressureCurve##OTHER##,EfficiencyCurve##OTHER##,OperationalCriteria##OTHER##,spProductQuantity##OTHER##,spTotalProductQuantity##OTHER##,RatedCurrent##ELECTRICAL_CURRENT##AMPERES,WarrantyContent##OTHER##,TotalPrimaryEnergyConsumption##OTHER##,WaterConsumption##OTHER##,MaintenanceSpecifications##OTHER##,AssessmentCondition##OTHER##,Type Comments##OTHER##,InsulationStandardClass##OTHER##,MaintenanceCertificate##OTHER##,ClimateChangePerUnit##OTHER##,spGenericalProductConfiguration##OTHER##,ClimateChange##OTHER##,spProductDescription##OTHER##,COBieCategory##OTHER##,spEasyVentProductDescription##OTHER##,ProductionYear##OTHER##,spSoundDistance##OTHER##,ApplicationOfFan##OTHER##,WaterConsumptionPerUnit##OTHER##,AtmosphericAcidificationPerUnit##OTHER##,AtmosphericAcidification##OTHER##,WheelTipSpeed##OTHER##,PA##LENGTH##MILLIMETERS,PB##LENGTH##MILLIMETERS,PC##LENGTH##MILLIMETERS,PD##LENGTH##MILLIMETERS,PF##LENGTH##MILLIMETERS,PH##LENGTH##MILLIMETERS,PK##LENGTH##MILLIMETERS,PL##LENGTH##MILLIMETERS
CVB-350/125 *230V50/60HZ* R6,0,125,0.4,0,5137282900,"B",5137282900,0,1700,0,0,0,0,0,http://easyvent.solerpalau.com/fan-info/view/00005/0/86/p/5137282900/1,http://www.solerpalau.com/,0,0,0,,,0,,,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,,,6.2,0,0,0,1,"8413893176554",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2020-12-31,0,0,0,0,2017-07-27,0,0,0,0,0,S&P Sistemas de Ventilación S.L.U.,0,0,0,0,0,0,0,0,0,0,0,0,125,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand S&P model CVB-350/125 *230V50/60HZ* R6 . ","IP44","8413893176554",0,0,0,0,0,0,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand [MARCA] model [MODELO] for an airflow [CAUDAL] and static pressure [PRESION]. ",0,0,0,CVB-350/125 *230V50/60HZ* R6,0,CVB-350/125 *230V50/60HZ* R6,0,CVB-350/125 *230V50/60HZ* R6,0,0,,0,0,0,0,308.5,213,315.5,125,97,93.7,340,271.6
CVB-600/150-160 *230V50/60HZ* R6,0,600,1.12,0,5137283700,"B",5137283700,0,2310,0,0,0,0,0,http://easyvent.solerpalau.com/fan-info/view/00005/0/86/p/5137283700/1,http://www.solerpalau.com/,0,0,0,,,0,,,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,,,7.3,0,0,0,1,"8413893176561",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2020-12-31,0,0,0,0,2017-07-27,0,0,0,0,0,S&P Sistemas de Ventilación S.L.U.,0,0,0,0,0,0,0,0,0,0,0,0,160,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand S&P model CVB-600/150-160 *230V50/60HZ* R6 . ","IP44","8413893176561",0,0,0,0,0,0,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand [MARCA] model [MODELO] for an airflow [CAUDAL] and static pressure [PRESION]. ",0,0,0,CVB-600/150-160 *230V50/60HZ* R6,0,CVB-600/150-160 *230V50/60HZ* R6,0,CVB-600/150-160 *230V50/60HZ* R6,0,0,,0,0,0,0,308.5,213,315.5,150,97,93.7,340,271.6
CVB-900/200 *230V50/60HZ* R6,0,900,0.75,0,5137284500,"B",5137284500,0,1100,0,0,0,0,0,http://easyvent.solerpalau.com/fan-info/view/00005/0/86/p/5137284500/1,http://www.solerpalau.com/,0,0,0,,,0,,,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,,,11,0,0,0,1,"8413893176578",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2020-12-31,0,0,0,0,2017-07-27,0,0,0,0,0,S&P Sistemas de Ventilación S.L.U.,0,0,0,0,0,0,0,0,0,0,0,0,200,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand S&P model CVB-900/200 *230V50/60HZ* R6 . ","IP44","8413893176578",0,0,0,0,0,0,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand [MARCA] model [MODELO] for an airflow [CAUDAL] and static pressure [PRESION]. ",0,0,0,CVB-900/200 *230V50/60HZ* R6,0,CVB-900/200 *230V50/60HZ* R6,0,CVB-900/200 *230V50/60HZ* R6,0,0,,0,0,0,0,431.1,246.5,421.1,200,118,117.7,445.6,394.2
CVB-1100/250 *230V50HZ* N6,0,1100,1.69,0,5137285200,"B",5137285200,0,1720,0,0,0,0,0,http://easyvent.solerpalau.com/fan-info/view/00005/0/86/p/5137285200/1,http://www.solerpalau.com/,0,0,0,,,0,,,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,,,11,0,0,0,1,"8413893176585",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,2020-12-31,0,0,0,0,2017-07-27,0,0,0,0,0,S&P Sistemas de Ventilación S.L.U.,0,0,0,0,0,0,0,0,0,0,0,0,250,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand S&P model CVB-1100/250 *230V50HZ* N6 . ","IP44","8413893176585",0,0,0,0,0,0,0,0,0,0,0,0,"Low profile fan manufactured from heavy gouge galvanised sheet steel, with melamine foam flame retardant acoustic insulaion M1. Suplied with a removable cover closing hermetically single inlet forward cuved impeller centrifugal fan with single phase external rotor motor. Remote terminal box. Brand [MARCA] model [MODELO] for an airflow [CAUDAL] and static pressure [PRESION]. ",0,0,0,CVB-1100/250 *230V50HZ* N6,0,CVB-1100/250 *230V50HZ* N6,0,CVB-1100/250 *230V50HZ* N6,0,0,,0,0,0,0,445.5,305,343.5,250,221.5,163.2,368,408.6
